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Installation of Fitpoint 
Installing the four corners 
When delivered in a closed truck the four corner exercises (Stepper, Twister, StepUp and BalanceBoard) will not be pre-assembled. 
[image: ][image: ]The necessary bolts, washers and lock nuts are supplied by Denfit
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1 - Put the Fitpoint on the wooden beams that come with the delivery (image 1) 
2 - Place the four corners in the right spot position (image 2)
3 - Tilt the floor backward and shove it over de pins  (image 3a and b)
4 - Lift the floor on side of the post so it is parallel with the Fitpoint floor (image 4)
5 - Push the bolt through the holes from the inside and screw on the lock nut from the other side (image 5a and b)
6 - Now the floor is installed (image 6)
7 - After the four corners are installed, remove the wooden beams
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Anchoring
The FitPoint has a weight of 1500 kg and therefor anchoring to the ground is not necessary. If anchoring is desirable, this is how it can be done:
 Step 3
Anchoring soft surface
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Step 1






[image: ]Anchoring on tarmac
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Anchoring on tarmac with chemical anchoring (not provided). Use drill instructions from your chemical anchoring

Anchoring on concrete
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Anchoring on concrete with wedge anchors. 
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